T-1 Day Until Showcase

* App works, nodes work
* Accelerometer generates interrupt (uses approx no power, so small it cannot be differentiated from noise)
  + Weird thing going on with the LED (needs to be on to get the
* Power board generates charge current- 10mA in direct sunlight
  + Tx every 4 sec w/o changing w/o changing charge state of batt
* Shade- charge current of .3mA
  + Tx every 4 mins w/o changing charge state of batt
* Does not work indoors (negative)
* 120+ m of range (did a range test from 90 deg statue to the inner loop)
  + Probably BLE starts doing something to compensate for lower SNR
* Need to reprint poster in Mudd Lab (oedk printer was running outta red toner)